ENVIRONMENTAL PROTECTION DIVISION PUBLIC NOTICE

WATERSHED PROTECTION BRANCH

March 13, 2020 Eatonton/Putnam County

Notice Issue Date City / County

April 13, 2020 BV-117-20-01

Notice Close Date Control Number

Eatonton-Putnam Water and Sewer Authority- Westside WWTF Improvements

Eatonton, GA 31024 (GPS Coordinates: 33.311945, -83.41147)

Activity

This notice is issued to inform the public of a receipt of an application for a variance submitted pursuant to a state environmental Law. The public is invited to comment during the 30-day period on the proposed activity. Site plans are available for review and are located in the following EPD office: Watershed Protection Branch, 200 Piedmont Avenue SW, Suite 418 West, Atlanta, GA 30334. Please contact Ms. Arnettia Murphy at (404) 656-4147 or email [arnettia.murphy@dnr.ga.gov](mailto:arnettia.murphy@dnr.ga.gov) to schedule an appointment to review the plans. Since the EPD has no authority to zone property or determine land use, only those comments addressing environmental issues related to air, water, and land protection will be considered in the application review process. Written comments should be submitted to: Program Manager, NonPoint Source Program, Erosion and Sedimentation Control, 2 Martin Luther King Jr. Drive SW, Suite 1462 East, Atlanta, GA 30334.

Type of Permit Application: Variance to encroach within the 25-foot State waters buffer. Applicable Law: Georgia Erosion and Sedimentation Act O.C.G.A. 12-7-1 et seq.

Applicable Rules: Erosion and Sedimentation Control Chapter 391-3-7

Basis under which variance shall be considered {391-3-7-.05 (2)(a-k)}: (a)

Description and Location of Proposed Activity:

This project will consist of upgrading the effluent pipe from 12-inch diameter to 16-inch diameter PVC. Additionally, a new headwall will be constructed to protect the pipe at the discharge point and a “doghouse” manhole will be constructed to connect the new lateral pipeline to the existing pipeline. All disturbed areas along the streambank will be stabilized with rolled erosion control products to cover 10 feet on both sides of the new pipe and revegetation along the slope. The proposed project will result in approximately 35 linear feet (612 square feet) of buffer disturbance lasting approximately 5 days located at an unnamed tributary of Little River, near Highway 441 and Monticello Road, in the Upper Oconee Watershed.

Name and Address of Permit Applicant: Mr. Freddie Wiggins

Wastewater Superintendent

Eatonton-Putnam Water and Sewer Authority

663 Godfrey Road

Eatonton, Georgia 31024

Summary of Rules Requirements for Variance Application:

The application for a variance must include an approved Erosion and Sediment Control Plan with control measures based on sound conservation and engineering practices which meet or exceed the standards in the "Manual for Erosion and Sediment Control in Georgia" and which will minimize erosion and deposition of sediments on adjacent lands or into State waters.

For Additional Information Contact: Victoria A. Adams, Environmental Specialist

EPD Watershed Protection Branch

NonPoint Source Program

2 Martin Luther King Jr. Drive SW, Suite 1462 East

Atlanta, GA 30334

Telephone: (404) 463-0003