**ENVIRONMENTAL PROTECTION DIVISION**

**DRAFT**

 **DEPARTMENT OF NATURAL RESOURCES**

 **STATE OF GEORGIA**

**PERMIT TO USE GROUNDWATER**

|  |
| --- |
| PERMIT NUMBER **New** DATE: **Month XX, 201X** |
| PERMIT HOLDER’S NAME **Wildwood Water, LLC** |
| PERMIT HOLDER'S ADDRESS  **1251 Twin Pines Drive, Greensboro, GA 30642 - Putnam County** |
| In accordance with the Provisions of the Groundwater Use Act, (O.C.G.A § 12-5-90 et seq.) as amended, and the Rules and Regulations for Groundwater Use, Chapter 391-3-2, promulgated pursuant thereto, this Permit is issued to withdraw, obtain, or utilize a maximum system wide total of groundwater in the amount of: **0.350** million gallons per day monthly average and **0.350** million gallons per day annual average; from **nine** well(s) located at **Greensboro, Georgia − Putnam County** for the purpose of a consumptive use for **a central water supply**. |
| This Permit is conditioned upon the permit holder complying with the following: **STANDARD CONDITIONS**(1) The provisions of the Groundwater Use Act, as amended, or any of the Rules and Regulations promulgated pursuant thereto;(2) The Permit must not be transferred except with the approval of the Georgia Environmental Protection Division (EPD);1. The Groundwater Withdrawal Report will be submitted MONTHLY in accordance with the following schedule:
* Production between the first day of the month and the last day of the month will be submitted to EPD by the 10th day of the following month (ex. January 1st through January 31st groundwater withdrawal data will be reported to the EPD by February 10th).

(4) The withdrawal of groundwater is limited to the quantities and purpose of the water herein specified. **SPECIAL CONDITIONS**1. This Permit is valid for ground water withdrawal from the **Crystalline Rock** Aquifer. No other aquifer(s) can be used without the approval of the EPD.
2. If multiple aquifers are designated in Special Condition (5) above, groundwater withdrawal of each aquifer must be reported separately. Each aquifer must be identified on the Groundwater Withdrawal Report, as well as listing the well or wells that are producing in each aquifer. If a well is producing in more than one aquifer, it is to be noted. The Groundwater Withdrawal Report must be submitted in accordance with the schedule outlined in Standard Condition (3) of this permit.
3. The replacement of any permitted well must receive prior approval from EPD.

And the additional attached conditions (8 through 13), which are hereby made a part of this Permit. |
|  In accordance with the application dated **July 15, 2014** and in conformity with the statements and supporting data entered therein or attached thereto, all of which are filed with the EPD and are hereby made part of this Permit.This permit is effective from the date first above written and is subject to revocation on evidence of noncompliance with any of the provisions of the Groundwater Use Act, as amended, or any of the Rules and Regulations promulgated pursuant thereto; or with any representation made in the above mentioned application or the statements and supporting data entered therein or attached thereto; or with any condition of this permit.Absent prior revocation in accordance with the above language, this Permit will expire on the **XXth day of Month, 202X.** |
| DIRECTOR'S SIGNATURE DATE: Director Environmental Protection DivisionMonth XX, 201X Department of Natural Resources |

STATE OF GEORGIA PAGE 2 OF 2

DEPARTMENT OF NATURAL RESOURCES PERMIT NO. New

ENVIRONMENTAL PROTECTION DIVISION DATE: Month XX, 201X

 **SPECIAL CONDITIONS**

1. This groundwater withdrawal permit and any future modifications or re-issuances of such, is conditional upon implementation of the Water Conservation Plan. This permit holder must demonstrate an effort to increase water use efficiency.
2. The permit holder must abide by applicable water conservation requirements.
3. The permit holder must abide by applicable drought response requirements.
4. In accordance with the Groundwater Use Rules, 391-3-2-.08(2), a permit holder will analyze a raw groundwater sample for specific conductance on an annual basis. Analysis for specific conductance must be conducted in accordance with 40 Code of Federal Regulations, Part 141.89. A raw groundwater sample must be collected for every five permitted wells (i.e., if you have between one and five permitted wells, collect one raw groundwater sample for analysis; if you have between six and ten permitted wells, collect a raw groundwater sample from two of the permitted wells, etc.). The groundwater samples will be collected from the highest yielding wells. The results must be submitted to EPD on corporate letterhead and will include the date sampled, well number, temperature of water sample at time of testing, the specific conductance result, and the units of measurement.
5. Due to the high percentage of the Non-Revenue Water reported, EPD requests the permit holder to submit a detailed annual progress report on efforts made to reduce the Non-Revenue Water within the system. The annual progress report should provide a description of implemented measures and how the implemented measures reduced the system’s Non-Revenue Water percentage.
6. This permit supersedes any and all previous permits of the same permit number.

 **PERMIT MODIFICATION**

The permit holder may seek modification of any of the terms of an unexpired permit upon written request to the Director. The Georgia EPD has the authority to modify any groundwater withdrawal permit at any time.